Data Hazard:

* Insert nops in code at compile time (WB-DC)
* Rearrange code at compile time
* Forward data at run time
* Stall the processor at run time